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Emergency Intercom


· 304 Stainless Steel body (SS316 available upon request)
· IP55-IP65 Waterproof rating
· Advanced noise reduction technology for HD calls
· Corrosion-resistant hardware
· CE, FCC, RoHS, IK10, IP65, ISO9001 standards
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MAIN FEATURES

Housed in stainless steel with a wire-drawing finish and manufactured to high standards, these telephones offer enhanced resistance to vandalism and ensure reliable communication at all times.
Additionally, this series of phones has been tested in salt spray and is highly durable in humid and corrosive environments. Extremely easy to install, the cable entrance is located at the back of the phone to prevent artificial damage.
Ideal for parking lots, lifts/elevators, hotels, doorways, railway/metro platforms, hospitals, police stations, ATMs, stadiums, and outdoor building etc.



· Hands-free operation with a single vandal-resistant metal button for emergency calls
· Equipped with an LED light that blinks during incoming calls
· Noise-cancelling microphone
· Built-in 2W speaker
· Flush mounted design with tamper-proof screws
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TECHNICAL SPECIFICATIONS

	SIP Specifications

	Power supply
	PoE powered or 12V DC powered

	Power adapter
	100~240VAC 50~60Hz / 12V DC

	Power consumption
	Idle 1W / Working 2.4W

	SIP protocol
	SIP 2.0 (RFC3261)

	Network port parameters
	WAN Port: 10/100Base- T RJ-45 for LAN, Auto MDIX，LAN Port: 10/100Base- T RJ-45 for PC, Auto MDIX

	Voice coders
	G.711 A/U, G.722 8000/16000, G.723, G.729

	Communication mode
	Full duplex

	Ringing volume
	90~95 dB (A) @ 1 meter

	Technical Specifications

	Compatible with most SIP-based IP-PBX servers that comply with SIP RFC 3261

	PoE 802.3af enabled (Power-over-Ethernet) or alternate power source

	PoE power supply, supports connecting the external loudspeakers (No external power supply needed)

	Supports automatic switching between primary and backup servers

	Supports remote Telnet debugging

	Supports two relays to remotely control external devices

	Operating temperature -40˚C to 65˚C / Storage temperature -40°C to 75°C

	M.T.B.F. exceeds 50,000 hours under normal operating conditions

	Network Web Management

	Fully configurable through any internet browser

	Static IP address provisioning or DHCP support

	Product self-diagnostic testing available through the web interface

	Network-adjustable earpiece volume and microphone sensitivity

	Firmware upload via web interface

	Echo cancellation: Supports G.168, and hands-free can support 96ms

	Supports SIP domain, SIP authentication (none, basic, MD5), and DNS name of server

	DTMF: SIPINFO, INBAND, RFC2833

	Dials Plan: Flexible dial-up configuration, support hotline

	Network Features

	WAN/LAN: Supports Bridge mode

	Supports static IP address

	Supports DHCP to obtain an IP address on WAN port

	Supports VLAN

	Supports web config

	Data Protocols: IPv4, TCP, UDP, ICMP, ARP, RTP, SRTP, ONVIF, SNMPv1, RTCP-XR, 802.1x, Static IP/DHCP IP Assignment,IEEE 802.1p/Q, QoS/ToS,
HTTP/HTTPS/DHCP, NTP, FTP/TFTP, CDP/LLDP VLAN Configuration, LDAP
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APPLICATIONCat5e
Cat5e


IP telephony system is an efficient and convenient communication solution that uses Internet connection to implement voice calls and other communication services. Compared with traditional telephone systems, IP telephone system has higher efficiency and conve- nience.Cat5e
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SIP Server
Cat5e
PoE Switch
Master station
Computer



OPTIONAL ACCESSORIES
Button
Multiple Options Available
JR-LP-02
LED Beacon Light
JR-HSA-10/20/25/30/35
Broadcast Horn
JR321-SC
Telephone Pillar
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APPLICATION SCENARIOS
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Metro	Airport

Platform

Elevator
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Clean room

Hospital

Bank

School


DIMENSIONS
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	Package

	Unit size
	216*146*40 (mm)

	Shipping dimensions
	250*180*80 (mm)

	Packaging materials
	Foam padding, carton

	Weight
	Gross weight: 2 kg / Net weight: 1.5 kg





Add: 4325 Woodland Park Dr. West Melbourne, Florida. 32904
Email: info@tuffcomm.com
Tel: +1 321-900-4599
Web: www.tuffcomm.com
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